[:SENSe]:W16E:TIME:RLENgth | command/query

Gets or sets the number of frames to acquire for a measurement.

Command Syntax: | [:SENSe]:W16E:TIME:RLENgth <value>
<value> | ::= | Integer number
Query Syntax: | [:SENSe]:W16E:TIME:RLENgth?
Returns | ::= | Integer number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.ResultLength

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |