# Win98SE USB Mass Storage Device Drivers

These drivers offer generic USB mass storage support for Windows 98SE. You should [check your version](http://www.technical-assistance.co.uk/kb/usbmsd98.php) of Win98 before installing. Once installed USB mass storage devices should work within Win98.

Version 3 of the drivers includes generic USB 2.0 controller drivers adding USB 2.0 support for computers that support it.

## To install the drivers

#### Version 3.x

1. Download the exe file to the desktop
2. Remove ALL drivers for USB flash drives in Device Manager
3. Remove ALL drivers for any USB 2.0 controllers (many have an uninstall option)
4. Remove ALL unknown devices from Device Manager
5. Run the exe file you downloaded, and follow the instructions, rebooting after installation
6. When the computer boots up again, it may detect new USB 2.0 controllers, in which case you may need to reboot again

If you do experience any problems, you can always try asking in our [forum](http://forum.technical-assistance.co.uk/).

## Download

The drivers can be downloaded from the following link:

## [**Windows 98 SE Generic USB Mass Storage Device Drivers v3.3 - nusb33e.exe**](http://www.technical-assistance.co.uk/drivers/nusb33e.exe)

## Related Forum Posts

1. [taskbar problem after loading nusb33e.exe](http://forum.technical-assistance.co.uk/taskbar-problem-after-loading-nusb33eexe-vt833.html)
2. [Need Help Installing Thumb Drive - Windows 98 FE](http://forum.technical-assistance.co.uk/need-help-installing-thumb-drive-windows-98-fe-vt824.html)
3. [Linking Win98SE and Vista Home](http://forum.technical-assistance.co.uk/linking-win98se-and-vista-home-vt812.html)
4. [inf file problem,cannot use usb ports, help please](http://forum.technical-assistance.co.uk/inf-file-problemcannot-use-usb-ports-help-please-vt799.html)
5. [Help with flash drive](http://forum.technical-assistance.co.uk/help-with-flash-drive-vt804.html)