G338xAA Agilent CTC Control for GC/MS ChemStation

Revision - A.01.05

Please read this information carefully. It is a supplement to the printed material you received with your software.

Contents

---------------------

1. CHN, JPN: Cycle Editor 'No license found' message is untranslated

2. Import Cycle Composer List (.psl) file always loads DEF_GC.s

3. GC ChemStation displays LC-Inj as an injection source

4. Initial install of CTC now loads default inject to: LC Vlv1 for GC

5. Copyright date on footer of CTC Welcome.htm is 2006

6. LC run time fixed at 10 minutes if no pump is configured.

7. Print Method dialog for CTC PAL Instrument has bars at end of text

1. CHN, JPN: Cycle Editor 'No license found' message is untranslated

CHN and JPN: Select Instrument\Cycle Editor when this is not installed. The pop-up that reads 'No license found!' is untranslated.

2. Import Cycle Composer List (.psl) file always loads DEF_GC.s

In GC ChemStation, load a valid sequence using CTC locations and methods. Select Sequence\Import CycleComposer List... Import a valid .psl file and OK. DEF_GC.s loads instead of the sequence currently loaded. Thus, you cannot append an imported .psl file to the desired sequence.

3. GC ChemStation displays LC-Inj as an injection source

On a GC ChemStation, select CTC PAL Edit Method. Available Cycles displays LC-Inj as a valid selection.

4. Initial install of CTC now loads default inject to: LC Vlv1 for GC

In the Cycle Arguments field, the default selection for Inject to is 'LC Vlv1' for a GC installation.

Change to a valid choice and this never returns.

5. Copyright date on footer of CTC Welcome.htm is 2006

Copyright date on footer of CTC Welcome.htm is 2006.

6. LC run time fixed at 10 minutes if no pump is configured

Due to the modular design of the 1200 Series LC, it could happen that a non-Agilent pump is integrated.

In this case, the run time of the complete LC system is always set to 10 minutes (defined by the Pal Inj).

The Pal overwrites settings from other LC modules (detector or column oven).

7. Print Method dialog for CTC PAL Instrument has bar characters at end of text

7890 with CTC A.01.03: Select File\Print Method. The text label in the Instrument/Acquisition field has two bars at the end of the text for the CTC PAL Instrument letters that replace the 'nt'.

NB:

Microsoft, MS and MS-DOS are registered trademarks of Microsoft Corporation.

Windows is a trademark of Microsoft Corporation.