Jan 2002

These three files, data.mdb, design.mdb, and server.exe are intended to be used exclusively with E7473A CDMA Drive Test, version A.09.02 to modify the software to work with Generic QCP CDMA phones.  This modification will allow QCP-2135, QCP-2235, and QCP-2255 to be recoginized as valid Phone resources.

To use:

1.  E7473A, version A.09.02 MUST be installed, but not currently running.
2.  Copy the three files found on this disk into the E74xx application folder, default path is "/Program Files/Agilent Technologies/E74xx".
3.  Change properties of data.mdb to uncheck the Read-only attributes of the file.
4.  Connect QCP phones to PC on desired COM ports.
5.  Start E7473A application, create new Database and use Auto Configure found under the Configuration context Hardware tab to create a new project.

If the phone is not found using Auto-Configure, reset the BAUD rate of the phone through the phone interface menu to 19200 and try auto-configure again.
